ESP configuration page |

GPIO management
GPIO | D0(16) | D1 (5) | D2 (4) | D3 (0) | D4 (2) | D5 (14) | D6 (12) | D7 (13) | D8 (14)
State |  |  |  |  |  |  |  |  |
Toggle |  |  |  |  |  |  |  |  |
Timer |  |  |  |  |  |  |  |  |
PWM |  |
| 0 |  |  |  | 1023
Global
MAC : | Channel : | Device name(4-20 caracters) | WiFi mode
Uptime : | RSSI : n/a |  |
sta | ap | both
BSSID : n/a |  | Disable module ? |
Access Point
WiFi name (4-20 caracters) |
WiFi key (8-20 caracters) |
Output power (0-20 dBm) | dBm
IP address |
Station
WiFi name (4-20 caracters) |  | IP configuration
WiFi key (8-20 caracters) |  |
dhcp | static
IP address | Netmask | Gateway | DNS
Apply configuration ? |  |
Commands